For Normal Strength Wastewater

For 1 Billion CFU/gram

1st Week = 25 lb for every 750,000 gallons every day

2nd Week = 25 lb for every 750,000 gallons every other day

3rd and 4th Week = 25 lb for every 750,000 gallons per week

For 5 Billion CFU/gram

1St Week = 5 Lbs for every 750,000 gallons every day

2nd Week = 5 Lbs for every 750,000 gallons every other day

3rd and 4th Week = 5 Lbs for every 750,000 per week.

For 10 Billion CFU/gram:

1st Week = 2.5 lb for every 750,000 gallons every day

2nd Week = 2.5 lb for every 750,000 gallons every other day

3rd and 4th Week = 2.5 lb for every 750,000 gallons per week.

For High Strength

MAINTENANCE

Need to evaluate if the 4th week dosage is appropriate. In most cases, a weekly dosage of 1-2 lb may be necessary depending on influent.